HOW TO UPGRADE DUNE HD MINI WITH OLD PRE-PRODUCTION FIRMWARE
============================================================

---------------------------------------------------------------------------

General information
===================

The first officially published/shipped Dune HD Mini firmare version is
081204_2147. If you have this firmware version of a newer firmware
version, you do not need this instruction.

If you have Dune HD Mini with an older firmware version, you have a
pre-production firmware version (and very likely a pre-production sample of
Dune HD Mini), and you need to follow this instruction.

How to determine my firmware version?
   - Check player setup: Setup / Information.

How to compare firmware versions?
   - The first 6 digits of the firmware version number specify the firmware
     date in the format YYMMDD, e.g.:
         081204 = 2008-12-04 (2008 december 04)

---------------------------------------------------------------------------

Upgrading from firmware versions older than 081128_2324
=======================================================

If you have Dune HD Mini with firmware version older than 081128_2324, i.e.
one of the following versions:

   081023_1938
   081020_1740
   081105_1820
   081119_1046

you should first upgrade to the following firmware version:

   081128_2324

using the following "transitional" DFF file:

   dune_firmware_081128_2324.dff

This DFF file is part of this upgrade package, available here:

   http://dune-hd.com/firmware/tmp/hdmini_upgrade_from_preproduction.zip

---------------------------------------------------------------------------

Upgrading from firmware version 081128_2324
===========================================

If you have Dune HD Mini with firmware version 081128_2324, you can upgrade
to any officially published Dune HD Mini firmware in the usual way (just
download the needed DFF file from http://hdi.co.il/firmware/hdmini and
launch it).

---------------------------------------------------------------------------
